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NAME：GW-9761 High Speed Parallel Winding Machine             

SPECIFICATION:
	Spindles
	1
	Spread Motor
	4-Phase stepping Motor

	Wire diameter
	0.02-0.8mm
	Max Speed
	6000rpm

	Spread Pitch
	0-9.999mm
	Memory
	999 Sequences

	Spread Width
	100mm（Max）
	Power Source
	AC 220V/110V±10%,50/60MHZ

	Winding Width
	150mm（Max）
	Weight
	45×67×10

	Main Motor
	1/2HP DC Motor
	Dimension
	45


FEATURES:

High Speed Parallel Winding Machine has microprocessor design ,easy for program-setting handing.

Wire guiding traverse shaft stepper motor with a constant-current driver offering fast wire guiding speed.

input the ‘Start Point’parameter by number key or teachable function ,and display the position of spreading head on the panel.
The wire of the High Speed Parallel Winding Machine runs though the nozzle of spreading head to arrange in order better.
The ceramic rollers for High Speed Parallel Winding Machine prevent enamel from high temperature.
ADVANTAGES:

The wireline shaft is driven by a stepping motor with a constant current circuit, with fast wireline speed and high precision.

The position of the winding point can be inputted by teaching, and the current position of the spool can be displayed.

High Speed Parallel Winding Machine adopts multi - wire rows, four different diameters can be installed at the same time.

Single machine can finish winding and insulation, acetic acid tape winding.

It can be replaced to make double axis synchronous winding machine.

PRODUCT:
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APPLICATION:
Typical applications for high torsion parallel spindle winding Machine with a single wire size, include the manufacture of gas ignition coils, solenoids, relays, motors and many forms of sensor coil in small and medium batch quantities.It is ideal for use in the production of small inductors, particularly bobbins wound with a single wire size and high turns count. The high maximum winding spindle speed (up to 6000 rpm) enables coils with a high turns count to be wound in a short cycle time.
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PRACTICAL APPLICATION :

TRAINNING CUSTOMER TO OPERATE WINDING MACHNE :
1.All service engineers with 10 years experience are gotten special technology training, who can deal with various breakdown problem.
2.Guide the user to use accurately and how to maintain the High Speed Winding Machine.
Provide free consultation about production process technology of electronic products.
3.In order to guarantee the machine used normally, we'd have training on how to operate, use and maintain our product by English manual, video, guiding on line.
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PACKAGING:

Packaging Material: Carton/Wooden case with foam inside.
1.General package(Paper carton or plastic bag): For small euipped parts for High Speed Winding Machine   
, Package it with form and pack paper to guarantee unbroken during the transport.
2.Wooden case package: For larger scale High Speed Winding Machine ,we have special skilled carpenter, who would make the proper wooden case with exact thickness,density,length. The up arrow ↑marked on the  outer wooden case. Buffer material would be put in the wooden case to prevent crack and shock.
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OPTIONAL ACCESSORIES

	NO.
	Item/Specification
	QUANTITY
	UNIT

	1 
	controller
	1
	PIECE

	2 
	winding motor
	1
	PIECE

	3 
	Spread motor
	1
	PIECE

	4 
	optical fiber sensor
	1
	PIECE

	5 
	B2-2.0 Inches shuttle
	1
	PIECE

	6 
	4 inches and 6 inches shuttle                                                           (base on machine model)
	1
	PIECE

	7 
	shuttle guide wheel
	1
	PIECE

	8 
	fixture head
	1
	PIECE

	9 
	green round belt                                                                                 (can send one free in orange)
	1
	M

	10 
	gear shape belt
	1
	Belt


FACTORY:

We-GREWIN INDUSTRIAL GROUP is expert in winding machines lines for 28Years. Our Grewin have ISO9001:2015,CE approvals,Machines'Patents,"high-tech enterprises"by the government.
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